|  |  |  |
| --- | --- | --- |
|  | **DECLARATION OF PERFORMANCE** | DoP Number |
| **DP.JGF.P001** |

|  |  |
| --- | --- |
| **1** | **Unique identification code of the product type** |
| 5460 Series Panic Exit Devices (Surface mounted) | |

|  |  |
| --- | --- |
| **2** | **Type, batch or serial number or any other element allowing identification of the construction** |
| 5460, 5462, 5464 | |

|  |  |
| --- | --- |
| **3** | **Intended use or uses of the construction product, in accordance with the applicable harmonized technical specification, as foreseen by the manufacturer** |
| For use on fire and smoke compartment doors and escape route doors, when fitted in accordance the manufacturers fitting instructions | |

|  |  |
| --- | --- |
| **4** | **Name, registered trade name or registered trade mark and address of the manufacturer required under Article 11(5)** |
| James Gibbons Format Limited, Neachells Lane, Wednesfield, Wolverhampton, WV11 3PU, United Kingdom | |

|  |  |
| --- | --- |
| **5** | **Where applicable, name and contract address of the authorised representative whose mandate covers the tasks specified in Article 12(2)** |
| N/A | |

|  |  |
| --- | --- |
| **6** | **System or systems of assessment and verification of constancy of performance of the construction product as set out in CPR, Annex V** |
| System 1 | |

|  |  |
| --- | --- |
| **7** | **In case of declaration of performance concerning a construction product covered by a harmonized standard** |
| EN1125:2008 Notified certification body No.1121 | |

|  |  |
| --- | --- |
| **8** | **European Technical Assessment** |
| N/A | |

|  |  |  |
| --- | --- | --- |
| **9** | **Declared Performance (Harmonised technical specification EN 1125:2008)** | |
| **Essential characteristics** | | **Performance** |
| Release Function | | Releases immediately (<1s) |
| Double Doorset | | Passed |
| Bar Installation | | <150mm |
| Bar Length | | ˃60% |
| Bar Projection | | Category 2 (≤100mm) |
| Operating Bar Face | | 32mm |
| Test Rod | | Passed |
| Door Face Gap | | ˃25mm |
| Top Vertical Bolt | | Passed (where applicable) |
| Keepers/Keeper dimensions | | Passed |
| Door mass & dimensions | | 200kg; 2350mm x 1230mm |
| Outside Access Device | | Passed |
| Release Forces | | ≤80N and ≤200N under pressure |
| Security Requirement | | Grade 2 |
| Corrosion Resistance | | Grade 3 (96 hours) |
| Lubrication | | Every 20,000 cycles |
| Re-engagement Force | | Passed (≤50N) |
| Durability | | 200,000 cycles |
| Abuse Resistance – Horizontal Bar/Vertical Rod | | Passed |
| Resistance to Fire (Integrity & insulation)  (for fire doors on escape routes)  Suitability of Panic Exit Devices for use on resisting doorset assemblies | | Grade B |
| Dangerous substances (Annex ZA3) | | The materials in the product(s) do not contain or release any dangerous substance in excess of the maximum levels specified in existing European material standards or any national standards. |

|  |  |
| --- | --- |
| **10** | **The performance of the product identified in points 1 and 2 is in conformity with the declared performance in point 9** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **This declaration of performance is issued under the sole responsibility of the manufacturer identified in point 4** | | | | | |
| *Signed for and on behalf of the manufacturer by:* | | | | | |
| **Inspected by (Print)** | **N.Brice** | **Signature** |  | **Date** | **5th August 2016** |